Product Support Bulletin

Subject: Decimal and ASCII Values for Variables

Date:  9/28/89                             PSB No:  

Page:  1 of 8                              Originator: RFB

The following list shows the ESC Codes that use a variable within a command. 

The ASCII characters 1 and 0, or their decimal or hexadecimal equivalent can

be used.  Most programs use the ASCII decimal equivalent as the method of

inserting codes.  However, some programs are restricted to using only decimal

values instead of the ASCII decimal equivalent.

Note: "*" Indicates the command is supported.

             Epson 9/24 Pin Printer Control Codes

赏屯屯屯屯屯屯屯屯屯屯屯送屯屯屯屯屯屯屯屯屯退屯屯屯退屯屯屯屯�

� FEATURE               � ESCAPE CODE        � 9 Pin � 24 Pin �

掏屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

� PITCH AND PROPORTIONAL SPACING                              �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Proportional On/Off   � ESC p n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪心哪哪哪哪哪哪哪哪哪男哪哪哪男哪哪哪哪�

� PRINT ENHANCEMENT                                           �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Select NLQ or Draft   � ESC x n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Expanded Print On/Off � ESC W n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Double High On/Off    � ESC w n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Underlining On/Off    � ESC - n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Select Super/Subscript� ESC S n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪心哪哪哪哪哪哪哪哪哪男哪哪哪男哪哪哪哪�

� USER DEFINED CHARACTER                                      �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Select Character Set  � ESC % n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪心哪哪哪哪哪哪哪哪哪男哪哪哪男哪哪哪哪�

� MISCELLANEOUS CODES                                         �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Unidirectional On/Off � ESC U n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Half Speed On/Off     � ESC s n            �   *   �   *    �

韧屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�  

                                               PSB No:

                                                Page:  2 of 8 

Only the decimal or hexadecimal values may be used for the command variable(s)

listed on the following pages.  For example, the command ESC k n in basic must be

expressed as CHR$(27)"k"chr$(0) or CHR$(&h1B)"k"CHR$(&h00) to select the Roman

font.

                Epson 9/24 Pin Printer Control Codes                  

赏屯屯屯屯屯屯屯屯屯屯屯送屯屯屯屯屯屯屯屯屯退屯屯屯退屯屯屯屯�

� FEATURE               � ESCAPE CODE        � 9 Pin � 24 Pin �

掏屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

� PRINT STYLE SELECTION                                       �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Select Font:          � ESC  k n           �   *   �   *    �

� n = 0 Roman           �                    �   *   �   *    �

� n = 1 San Serif       �                    �   *   �   *    �

� n = 2 Courier         �                    �       �   *    �

� n = 3 Prestige        �                    �       �   *    �

� n = 4 Script          �                    �       �   *    �

� n = 5 Ocr-B           �                    �       �   *    �

� n = 6 Ocr-A           �                    �       �   *    �

� n = 7 Orator 哪目    谧 Available only with�       �   *    �

� n = 8 Orator S 馁    雷 Multi-Font Module  �       �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Character Style:      � ESC q n            �       �   *    �

� n = 0 Normal          �                    �       �   *    �

� n = 1 Outline         �                    �       �   *    �

� n = 2 Shadow          �                    �       �   *    �

� n = 3 Outline & Shadow�                    �       �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Master Select:        � ESC  ! n           �   *   �   *    �

� n =    0 Pica         �                    �   *   �   *    �

� n =    1 Elite        �                    �   *   �   *    �

� n =    2 Proportional �                    �   *   �   *    �

� n =    4 Condensed    �                    �   *   �   *    �

� n =    8 Emphasized   �                    �   *   �   *    �

� n =   16 Double Strike�                    �   *   �   *    �

� n =   32 Double Wide  �                    �   *   �   *    �

� n =   64 Italic       �                    �   *   �   *    �

� n =  128 Underline    �                    �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Select Score:         � ESC ( - n1 n2 m d1 �       �   *    �

� n1 Must be 3          � d2                 �       �   *    �

� n2 Must be 0          �                    �       �   *    �

�  m Must be 1          �                    �       �   *    �

� d1 = 1 Underscore     �                    �       �   *    �

� d1 = 2 Strike-Through �                    �       �   *    �

� d1 = 3 Overscore      �                    �       �   *    �

� d2 = 0 Cancel Selected�                    �       �   *    �

�        Score          �                    �       �        �

� d2 = 1 Single Line    �                    �       �   *    �

�        Continuous     �                    �       �        �

韧屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

                                                 Page:  3 of 8 

                Epson 9/24 Pin Printer Control Codes

赏屯屯屯屯屯屯屯屯屯屯屯送屯屯屯屯屯屯屯屯屯退屯屯屯退屯屯屯屯�

� FEATURE               � ESCAPE CODE        � 9 Pin � 24 Pin �

掏屯屯屯屯屯屯屯屯屯屯屯瓮屯屯屯屯屯屯屯屯屯臀屯屯屯臀屯屯屯屯�

� Select Score:         � ESC (- n1 n2 m d1  �       �   *    �

� (continued)           � d2                 �       �        �

� d2 = 2 Double Line    �                    �       �   *    �

�        Continuous     �                    �       �        �

� d2 = 5 Single Line    �                    �       �   *    �

�        Broken         �                    �       �        �

� d2 = 6 Double Line    �                    �       �   *    �

�        Broken         �                    �       �        �

悄哪哪哪哪哪哪哪哪哪哪哪心哪哪哪哪哪哪哪哪哪男哪哪哪男哪哪哪哪�

� LINE SPACING                                                �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� n/360-inch Spacing    � ESC + n            �       �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� n/180-inch Spacing    � ESC 3 n            �       �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� n/216-inch Spacing    � ESC 3 n            �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� n/60-inch Spacing     � ESC A n            �       �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� n/72-inch Spacing     � ESC A n            �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪耗哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Immediate n/216 Feed  � ESC J n            �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Immediate n/180 Feed  � ESC J n            �       �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Reverse Feed n/216    � ESC j n            �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Reverse Feed n/180    � ESC j n            �       �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪心哪哪哪哪哪哪哪哪哪男哪哪哪男哪哪哪哪�

� PAGE FORMATTING                                             �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Immediate Mode On/Off � ESC i n            �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Intercharacter Spacing� ESC SP n           �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Page Length in Lines  � ESC C n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Page Length in Inches � ESC C NUL n        �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Skip Over Perforation � ESC N n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Set Left Margin       � ESC l n            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Set Right Margin      � ESC Q n            �   *   �   *    �

韧屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

                                                PSB No: 

                                                 Page:  4 of 8

                Epson 9/24 Pin Printer Control Codes

赏屯屯屯屯屯屯屯屯屯屯屯送屯屯屯屯屯屯屯屯屯退屯屯屯退屯屯屯屯�

� FEATURE               � ESCAPE CODE        � 9 Pin � 24 Pin �

掏屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

� HORIZONTAL TAB SETTING                                      �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Horizontal Tab        � HT                 �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Horizontal Tab Stops  � ESC D n1 n2..NUL   �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Set Tab Increment     � ESC e NUL n        �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� SET HTabs in Spaces   � ESC f NUL n        �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪心哪哪哪哪哪哪哪哪哪男哪哪哪男哪哪哪哪�

� VERTICAL TAB SETTING                                        �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Set Tab Stops         � ESC B n1 n2..NUL   �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Set VFU Tab Channel   � ESC b x n1 n2..NUL �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Select VFU Tab Channel� ESC / x            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Set Tab Increment     � ESC e 1 n          �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Vertical Skip         � ESC f 1 n          �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Set VTabs in Channel  � ESC b c n1 n2...NUL�   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Set VTab Channel      � ESC / n            �   *   �   *    �

韧屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

                                                PSB No:

                                                 Page:  5 of 8

                Epson 9/24 Pin Printer Control Codes                  

赏屯屯屯屯屯屯屯屯屯屯屯送屯屯屯屯屯屯屯屯屯退屯屯屯退屯屯屯屯�

� FEATURE               � ESCAPE CODE        � 9 Pin � 24 Pin �

掏屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

� GRAPHICS                                                    �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Select Graphic Mode   � ESC  * m n1 n2 data�   *   �   *    �

� 8-Pin Graphics:       �                    �       �        �

� m = 0   60 DPI        �                    �   *   �   *    �

� m = 1  120 DPI        �                    �   *   �   *    �

� m = 2  120 DPI Hi Spd �                    �   *   �   *    �

� m = 3  240 DPI        �                    �   *   �   *    �

� m = 4   80 DPI        �                    �   *   �   *    �

� m = 5   72 DPI        �                    �   *   �        �

� m = 6   90 DPI        �                    �   *   �   *    �

� m = 7  144 DPI        �                    �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Select Graphics Mode  � ESC * m n1 n2 data �       �   *    �

� 24-Pin Graphics:      �                    �       �        �

� m = 32   60 DPI       �                    �       �   *    �

� m = 33  120 DPI       �                    �       �   *    �

� m = 38   90 DPI       �                    �       �   *    �

� m = 39  180 DPI       �                    �       �   *    �

� m = 40  360 DPI       �                    �       �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪心哪哪哪哪哪哪哪哪哪男哪哪哪男哪哪哪哪�

� Individual Graphics Commands                                �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Single-Density 60 DPI � ESC K n1 n2 data   �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Double-Density 120 DPI� ESC L n1 n2 data   �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Hi-Speed Dbl. 120 DPI � ESC Y n1 n2 data   �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Quad. Density 240 DPI � ESC Z n1 n2 data   �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� 9-Pin 60 DPI          � ESC ^ 0 n1 n2 data �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� 9-Pin 120 DPI         � ESC ^ 1 n1 n2 data �   *   �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Reassign Graphics Mode� ESC ? n            �   *   �        �

韧屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

                                                PSB No:

                                                 Page:  6 of 8

                Epson 9/24 Pin Printer Control Codes                  

赏屯屯屯屯屯屯屯屯屯屯屯送屯屯屯屯屯屯屯屯屯退屯屯屯退屯屯屯屯�

� FEATURE               � ESCAPE CODE        � 9 Pin � 24 Pin �

掏屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

� USER DEFINED CHARACTERS                                     �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Define User Defined   � ESC & NUL n1 n2 a1 �       �        �

� Character             � data               �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Copy ROM to RAM       � ESC : NUL NUL NUL  �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Copy ROM to RAM       � ESC : NUL n NUL    �   *   �   *    �

� n = 0 Roman           �                    �       �        �

� n = 1 San Serif       �                    �       �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Select ROM CG         � ESC % 0            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Select Download CG    � ESC % 1            �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪心哪哪哪哪哪哪哪哪哪男哪哪哪男哪哪哪哪�

� JUSTIFICATION                                               �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪� 

� Justification:        � ESC a n            �   *   �   *    �

�                       �                    �       �        �

� n = 0 Flush Left      �                    �   *   �   *    �

� n = 1 Centering       �                    �   *   �   *    �

� n = 2 Flush Right     �                    �   *   �   *    �

� n = 3 Justified       �                    �   *   �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪心哪哪哪哪哪哪哪哪哪男哪哪哪男哪哪哪哪�

� SELECT CHARACTER TABLE                                      �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Select Character Set: � ESC t n            �   *   �   *    �

�                       �                    �       �        �

� n = 0 Italic set      �                    �   *   �   *    �

� n = 1 Graphic set     �                    �   *   �   *    �

� n = 2 User-Defined Set�                    �       �   *    �

�       Remap to 80h-FFh�                    �       �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Printable Code Area   � ESC I n            �   *   �        �

� Expansion:            �                    �       �        �

� n = 0 Restore Codes   �                    �       �        �

� n = 1 Redefine Codes  �                    �       �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Select International  � ESC R n            �   *   �   *    �

� Character Set:        �                    �       �        �

�                       �                    �       �        �

� n = 0 USA             �                    �       �        �

� n = 1 France          �                    �       �        �

� n = 2 Germany         �                    �       �        �

� n = 3 United Kingdom  �                    �       �        �

韧屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

                                                PSB No:

                                                 Page:  7 of 8

                Epson 9/24 Pin Printer Control Codes                  

赏屯屯屯屯屯屯屯屯屯屯屯送屯屯屯屯屯屯屯屯屯退屯屯屯退屯屯屯屯�

� FEATURE               � ESCAPE CODE        � 9 Pin � 24 Pin �

掏屯屯屯屯屯屯屯屯屯屯屯瓮屯屯屯屯屯屯屯屯屯臀屯屯屯臀屯屯屯屯�

� Select International  � ESC R n            �   *   �   *    �

� Characters (continued)�                    �       �        �   

�                       �                    �       �        �

� n =  4 Denmark I      �                    �   *   �   *    �

� n =  5 Sweden         �                    �   *   �   *    �

� n =  6 Italy          �                    �   *   �   *    �

� n =  7 Spain          �                    �   *   �   *    �

� n =  8 Japan          �                    �   *   �   *    �

� n =  9 Norway         �                    �   *   �   *    �

� n = 10 Denmark II     �                    �   *   �   *    �

� n = 11 Spain II       �                    �   *   �   *    �

� n = 12 Latin America  �                    �   *   �   *    �

� n = 13 Korea          �                    �       �   *    �

� n = 64 Legal          �                    �       �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪心哪哪哪哪哪哪哪哪哪男哪哪哪男哪哪哪哪�

� OTHER CONTROL CODES                                         �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Set Absolute Print    � ESC $ n1 n2        �   *   �   *    �

� Position              �                    �       �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Set Relative Print    � ESC \ n1 n2        �   *   �   *    �

� Position              �                    �       �        �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Repeat Data           � ESC V n data       �       �   *    �

悄哪哪哪哪哪哪哪哪哪哪哪啄哪哪哪哪哪哪哪哪哪淖哪哪哪淖哪哪哪哪�

� Color Selection:      � ESC r n            �   *   �   *    �

�                       �                    �       �        �

� n = 0 Black           �                    �   *   �   *    �

� n = 1 Red (Magenta)   �                    �   *   �   *    �

� n = 2 Blue (Cyan)     �                    �   *   �   *    �

� n = 3 Violet          �                    �   *   �   *    �

� n = 4 Yellow          �                    �   *   �   *    �

� n = 5 Orange          �                    �   *   �   *    �

� n = 6 Green           �                    �   *   �   *    �

韧屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

                                                PSB No:

                                                 Page:  8 of 8

The following command uses the ASCII character decimal value only.

                Epson 9/24 Pin Printer Control Codes                  

赏屯屯屯屯屯屯屯屯屯屯屯送屯屯屯屯屯屯屯屯屯退屯屯屯退屯屯屯屯�

� FEATURE               � ESCAPE CODE        � 9 Pin � 24 Pin �

掏屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

� CUT SHEET FEEDER CONTROL                                    �

悄哪哪哪哪哪哪哪哪哪哪哪夷哪哪哪哪哪哪哪哪哪囊哪哪哪囊哪哪哪哪�

� Cut Sheet Feeder      � ESC EM n           �       �        �

� Operation:            �                    �   *   �   *    �

�                       �                    �       �        �

� n = 0 Disable CSF     �                    �   *   �   *    �

� n = 1 Select Bin 1    �                    �   *   �   *    �

� n = 2 Select Bin 2    �                    �   *   �   *    �

� n = 4 Enable CSF      �                    �   *   �   *    �

� n = R Eject Sheet     �                    �   *   �   *    �

韧屯屯屯屯屯屯屯屯屯屯屯释屯屯屯屯屯屯屯屯屯褪屯屯屯褪屯屯屯屯�

It is urged that a functional understanding of the printer commands be obtained. 

Reference to the User's Manual is encouraged whenever a more detailed command

description is desired.  Some of the commands listed are unique to certain printers. 

For a detailed listing of the commands supported by a specific printer, please refer to

the Command Summary in the printer's User's Manual or the Control Code Matrix

chapter in the Epson Programmers Reference Manual.  The Programmers Reference

Manual can be ordered from Epson Accessories Sales under Part No. : PTM-0.

Note:    If a particular command is not listed in the printer's Users

         Manual, the command is not supported.